Public Tender no. 027/2026 – Annex C

Initial Proposal Form

for submission by email to cnbe.contract@marinha.mil.br
	Company Details

	Company’s name
	
	NCAGE:
 


	Address
	
	

	Telephone
	
	Email
	
	


	Item
	NSN
	Description
	Unit
	Quantity
	Unit Price
	Total Price
	Currency
	Note

	1
	6145-99-521-8267
	Single-core flexible shore supply cable, suitable for reeling applications, Class 5 tinned copper conductor, rated voltage 0.6/1 kV, insulation in thermoset elastomeric compound (EPR) for 90°C, outer sheath in heavy-duty marine elastomeric compound, black colour, certified for flexible/dynamic operation (Type WM / Reeling), 240 mm² cross- sectional area.
	M
	2.966,4
	
	
	
	

	2
	6145

-99-

521-

8263
	Single-core flexible shore supply cable, suitable for reeling applications, Class 5 tinned copper conductor, rated voltage 0.6/1 kV, insulation in thermoset elastomeric compound (EPR) for 90°C, outer sheath in heavy-duty marine elastomeric compound, black colour, certified for flexible/dynamic operation (Type WM / Reeling), 95 mm² cross- sectional area.
	M
	247,2
	
	
	
	


I hereby confirm that:
I am fully aware of the necessary conditions for the preparation of the proposal and for the delivery of the object in compliance with the Terms and Conditions set forth in Public Tender No. 027/2026 and its Annexes;
The prices offered for each item include all charges provided for in the Tender Notice, including freight, labeling, packaging, insurance, and certificate of conformity.
Name/ Position:
Date:
Signature:
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